**DOCUMENT No. 1**

**ADMISSION APPLICATION FORM**

(to be drawn up on the manufacturer’s letterhead)

Letter addressed to: **CERTIGAZ**

*ftao General Director*

Immeuble le Linéa

1, rue du Général Leclerc

CS 60254

F – 92047 PARIS LA DEFENSE

Subject: Application for admission (initial, by maintenance, extension) to the ATG Sertissage Mark applicable to copper press fittings for use on gas installations.

Dear Sir,

I request permission to affix the ATG-Sert Mark on the products that I manufacture, in accordance with the applicable specifications which characteristics can be found in annex.

I declare that I have read the aforementioned texts, the ATG-Sert Certification Rules.

I agree:

- to comply fully with the requirements of the Certification Rules, as well as with the decisions taken or to be taken, in execution of said requirements;

- to sell products bearing the ATG-Sertissage Mark only after taking all the precautions to ensure their compliance with standards and specifications;

- to reserve the Mark and the reference of the products submitted to the ATG-Sertissage Mark only to the fittings conforming to those certified;

- to take all measures to protect the trademark submitted to the ATG-Sertissage Mark in order to have an exclusive right to this Mark under the industrial property legislation;

- to affix the Mark, unequivocally, on the certified products and only on them;

- to carry out the in-process controls required under the Rules of Certification of the Mark;

- to report without delay to CERTIGAZ any incident, any modification to the manufacturing method or organisation, and more generally, any fact likely to cause a variation from the conditions in which the Mark was granted;

- to facilitate the task of auditors mandated by CERTIGAZ within the framework of their missions;

**DOCUMENT No. 1**

- to provide any supporting documents required for the application of a penalty;

- to provide the products designated by CERTIGAZ free of charge for verifications and send them at my expense and under my responsibility to the laboratory designated by CERTIGAZ;

- to pay the amount of the costs for examination of the application laid down in the financial framework of the Mark, and to make any subsequent payments that may be claimed in accordance with the rules of the Mark;

- not to indicate on each and every printed advertisements or catalogues, characteristics other than those which are confirmed by the tests and which will be communicated.

(2) I also authorise the company ............................................... (3) represented by Mr................................... (name and capacity) to represent me on French territory for all issues relating to the use of the ATG-Sertissage Mark.

(2) I consequently request that the expenses that are to be borne by me be invoiced directly to the said representative. This agent will ensure immediate settlement of invoices upon receipt on my behalf as bound so to do in accepting to represent me.

(2) I undertake to inform CERTIGAZ immediately of any appointment of a new agent replacing the above-mentioned agent.

Yours faithfully,

*Date*

*Seal and signature of* ***the******representative***(4)(5) *Seal and signature of* ***the applicant***(4)(5)

*Seal and signature of* ***the manufacturer*** (6)

Enclosures : General information form;

Product identification form;

Technical file(s).

(2) Optional. This paragraph only concerns applicants located outside European territory (EEE and AELE)

(3) The designation of the agent company shall include: corporate name, form of the company, registered office, trade register number, to be entered on Document no. 2

(4) The signatures of the applicant and its representative in European territory (EEE and AELE) must be preceded by the handwritten words “*Approved for representation*” and “*Approved for acceptance of representation*”, respectively

(5) Signature preceded by the handwritten words “*Read and approved*”

(6) In the case of the application by maintenance

**DOCUMENT No. 2**

**GENERAL INFORMATION FORM**

**• Company name and address of the applicant:**

Contact person: Telephone: Fax:

Email:

Information for billing (VAT no., SIRET):

**•** Where applicable, **name and address of the agent in France:**

Contact person: Telephone: Fax:

Email:

Information for billing (VAT no., SIRET):

**• Company name(s) and address(es) of the manufacturing unit(s):**

§ to be duplicated if multiple sites are concerned

Contact person: Telephone: Fax:

Email:

**•** **Company name and address of the packaging unit** (if ≠ from the manufacturer):

§ to be duplicated if multiple sites are concerned

Contact person: Telephone: Fax:

Email:

**• Company name and address of the fitting supplier** (if resold)**:**

§ to be duplicated if multiple sites are concerned

Contact person: Telephone: Fax:

Email:

**• Company name and address of the site performing the release tests:**

§ to be duplicated if multiple sites are concerned

Contact person: Telephone: Fax:

Email:

**DOCUMENT No. 3**

**FITTING IDENTIFICATION FORM**

(To be attached to the technical file)

# Trademark:

# Trade reference:

# Types and sizes of fittings:

Insert or attach a table in excel format as shown in the model below, duly completed

# Specification of copper tubes (grade R220 - R250 - R290, thickness and diameter):

In the unshaded cells, Mark with a cross the copper tubes compatible according to Standard NF EN 1057 and Specifications ATG B.524 in accordance with the ATG-Sert Rules. These tubes are NF certified according to the NF090 Mark.

|  |  |  |
| --- | --- | --- |
| **State** | **Thickness** | **Diameter** |
| **12** | **14** | **15** | **16** | **18** | **22** | **28** | **35** | **42** | **54** |
| **R220** | **1** |  |  |  |  |  |  |  |  |  |  |
| **R250** | **0,8** |  |  |  |  |  |  |  |  |  |  |
| **R250** | **1** |  |  |  |  |  |  |  |  |  |  |
| **R290** | **1** |  |  |  |  |  |  |  |  |  |  |
| **R290** | **1.2** |  |  |  |  |  |  |  |  |  |  |
| **R290** | **1.5** |  |  |  |  |  |  |  |  |  |  |

Dimensions in mm

# Seal characteristics (attach certificates):

- Nature (elastomer family):

- Supplier :

- Reference (standard designation and reference standard):

- Hardness:

- Temperature range:

- Colour:

Note: The TGA characterisation test on the seal according to ISO 9924-2 may be provided.

# Fitting raw materials (standard designation and reference standard):

# Crimping type: [ ]  Single [ ]  Double

# Tool(s) recommended for crimping:

Attach any additional document designating the tool and its use.

Complete the table on the next page for the various tools.